**GIBBONS 1.5HP BLOWER SPECIFICATIONS**

Usage Bouncy Castle Fans, Fans for Inflatable Obstacle Courses, Fans for Inflatable Sport Units

Material Galvanised Steel Sheet

Rated input power 1.68kW

Rated ouput power 1.1kW

Horsepower 1.50Hp

Motor type TE

Motor phase AC

Voltage 220-240v

Frequency 50Hz

Starting current 22A

Max running current 7.3/7.0A

Capacitor type 25µF

Insulation class F

Maximum motor speed 2800 rpm

Performance @ 4"wg 1050 cfm

Performance @ 1000 pa 1784 m3/hr

IP rating fan 55

Maximum power 44

Weight 16.6Kg / 36.6lbs

Product dimensions 41cm x 22cm x 53cm / 16.113'' x 8.646'' x 20.829''

Packaging dimensions 46cm x 28cm x 53cm / 18.078'' x 11.004'' x 20.829''

Plug type CEE Form Plug, 2P+E, 16A

Decibel level @ 5M 83dBA

Power supply Single Phase

Casing type Metal

Inflatable size Up to 8M x 8M (24ft x 24ft)

- See more at: [http://www.gibbonsfans.com/uk/electric-fans/inflatable-blower-fp5005-15-hp-230v-50hz/#sthash.oPSL5FBe.dpuf](http://www.gibbonsfans.com/uk/electric-fans/inflatable-blower-fp5005-15-hp-230v-50hz/%22%20%5Cl%20%22sthash.oPSL5FBe.dpuf%22%20%5Ct%20%22_blank)